**Annex 8.1.5a**

|  |
| --- |
| **PERMIT TO WORK: Commercial Diving Operations** |

|  |
| --- |
| A permit for commercial diving must be issued by the Harbour Master or one of the Assistants every time a commercial dive takes place within the RYHA area of jurisdiction. The validity of the permit must not exceed 12 hours |

|  |
| --- |
| Date Dive start time Dive finish time |

|  |
| --- |
| To Undertake the specific works of: |

|  |  |
| --- | --- |
| Name and address of diving contractor | Contact numbersMobile:Land:  |
| Dive supervisor:  | Low water: |
| Number of divers: | Area of dive: |

|  |
| --- |
| **RYHA requirements** |
| * Code flag A should be displayed whenever a diver is in the water.
* A second person onboard should be nominated as a safety lookout, while divers are in the water and monitor VHF CH16.
* Risk assessment should be available for inspection
* Method statement should be available for inspection
* Weather conditions are suitable
* Notification to public of diving activities displayed on access pontoon
 |
| **The dive will be conducted under relevant HSE ACOP requirements and the Diving Operations at Work Regulations (1997) the contents of which I am aware of:**Dive Supervisor: Date: |
| Approval to conduct diving operations within the limits of this permitHarbour Master: Date: |
| **Post Dive Requirements**  |
| Dive Completed; Time: Date: Dive Supervisor Signature:Harbour Office/Master informed dive completed – email/txt/phone |